PREVIOUS | INDEX | NEXT

1 BULB (NS)
2 LABEL, FUSE
3 BEAM COMP., STEERING HANGER
4 BEAM COMP., STEERING HANGER CENTER
5 STOPPER, GLOVE BOX LID
6 STOPPER, GLOVE BOX LID
7 CAP, INSTRUMENT PANEL STAY
8 LOCK, FUSE PANEL
9 SPRING, FUSE PANEL
10 NUT, CENTER PANEL
11 PANEL ASSY., INSTRUMENT *NH167L*
11 PANEL ASSY., INSTRUMENT *NH89L*
12 CUSHION, INSTRUMENT PANEL
13 SEAL, FR. INSTRUMENT PANEL
14 SEAL, SIDE DEFROSTER (A)
15 LID ASSY., SIDE FIX *NH89L*
15 LID ASSY., SIDE FIX *NH167L*
16 BRACKET, R. INSTRUMENT SIDE
17 BRACKET, L. INSTRUMENT SIDE
18 FRAME COMP., INSTRUMENT CENTER
19 STAY, CENTER OUTLET
20 GARNISH ASSY., METER VISOR *NH167L*
20 GARNISH ASSY., METER VISOR *NH89L*
21 BRACKET, R. VISOR LOWER
22 BRACKET, L. VISOR LOWER
23 COVER, METER VISOR *NH167L*
23 COVER, METER VISOR *NH89L*
24 BRACKET, R. METER
25 BRACKET, VISOR COVER
26 BRACKET, L. METER
27 COVER, INSTRUMENT PANEL DRIVER LOWER *NH89L*
27 COVER, INSTRUMENT PANEL DRIVER LOWER *NH167L*
28 HARNESS ASSY., LAMP
29 LID, R. INSTRUMENT PANEL LOWER *NH89L*
29 LID, R. INSTRUMENT PANEL LOWER *NH167L*
30 LID, L. INSTRUMENT PANEL LOWER *NH89L*
30 LID, L. INSTRUMENT PANEL LOWER *NH167L*
31 GARNISH ASSY., R. FR. DEFROSTER *NH89L*
31 GARNISH ASSY., R. FR. DEFROSTER *NH167L*
32 GARNISH ASSY., L. FR. DEFROSTER *NH167L*
32 GARNISH ASSY., L. FR. DEFROSTER *NH89L*
33 GARNISH ASSY., R. SIDE DEFROSTER *NH89L*
33 GARNISH ASSY., R. SIDE DEFROSTER *NH167L*
34 GARNISH ASSY., L. SIDE DEFROSTER *NH89L*
34 GARNISH ASSY., L. SIDE DEFROSTER *NH167L*
35 OUTLET ASSY., FRESH AIR *NH1L*
38 POCKET ASSY., COIN *NH89L*
38 POCKET ASSY., COIN *NH167L*
39 KNOB, FUSE LID
40 LABEL, COIN
41 SCREW, TAPPING, 4X12
42 SCREW, TAPPING, 4X16
43 BOLT-WASHER, 6X25
44 NUT, SPRING, 4MM
45 E-RING, 4MM
46 NUT, NYLON, 3MM
47 NUT, NYLON, 3MM
48 GROMMET, SCREW, 5MM (WHITE)
49 CLIP, FITTING
50 GROMMET, SCREW, 5MM
51 BOLT-WASHER, 6X16
52 BOLT-WASHER, 6X16
53 BOLT-WASHER, 8X20
54 SCREW, TAPPING, 4X12
55 WASHER, PLAIN, 6MM