PREVIOUS | INDEX | NEXT

1 JOINT B, WASHER TUBE (MITSUBA)
2 JOINT, TUBE
3 HOOD COMP.
4 HINGE COMP., R. HOOD
5 STOPPER, R. HOOD HINGE
6 STOPPER, L. HOOD HINGE
7 HINGE COMP., L. HOOD
8 COWL COMP., FR. TOP
9 SHELTER, AIR CONDITIONER
10 GROMMET, HOOD WIRE
11 HOOK, SIDE LINING
12 LOCK ASSY., HOOD
13 WIRE COMP., HOOD
14 LEVER ASSY., HOOD WIRE *NH89L*
14 LEVER ASSY., HOOD WIRE *NH167L*
16 RUBBER, HOOD SEAL
17 RUBBER, RR. HOOD SEAL
18 CUSHION, HOOD
19 STAY, HOOD OPENER
20 CUSHION, HOOD SIDE
21 CUSHION B, HOOD STOPPER
22 MOLDING, HOOD PROTECTOR
23 PROTECTOR, HOOD SIDE
24 GARNISH, HOOD
25 GROMMET, SCREW, 4MM
26 NOZZLE, R. WINDSHIELD WASHER
27 NOZZLE, L. WINDSHIELD WASHER
28 BOLT-WASHER, 6X15
29 SCREW-WASHER, TAPPING, 4X12
30 SCREW-WASHER, 5X8
31 BOLT-WASHER, 6X16 (DACRO COATING)
32 HOLDER, HOOD OPENER STAY
33 PLUG, HOOD HOLE
34 CLIP, TUBE, 7MM
35 CLIP, SIDE APRON MOLDING
36 GROMMET, HOOD STAY
37 CLIP, HOOD GARNISH
38 CLIP, AIRSCOOP GRILLE (BLACK)
40 CLIP, HOOD SEAL
41 CLIP, HOOD WIRE
42 BOLT-WASHER, 6X16
43 SCREW, TAPPING, 4X16
44 TUBE, VINYL, 4X7X210 (95003-07001-60M)
45 TUBE, VINYL, 4X7X330 (95003-07001-60M)
46 TUBE, VINYL, 4X7X420 (95003-07001-60M)
47 PLUG, BLIND, 18MM