PREVIOUS | INDEX | NEXT

1 BLOCK ASSY., CYLINDER
2 CAP, SEALING, 35MM
3 BOLT, SEALING, 14MM
4 JOINT, OIL COOLER
5 SEAL, TIMING RUBBER
6 PIPE, OIL LEVEL
7 STAY, OIL LEVEL PIPE
8 BOLT, SEALING, 22MM
9 BRIDGE COMP., BEARING CAP
10 PAN COMP., OIL
11 PLATE, BAFFLE
12 GASKET, OIL PAN
13 COVER, R. SIDE
14 BRACKET, ENGINE MOUNTING
15 STIFFENER, FR. ENGINE
16 WASHER, SEALING BOLT
17 ORIFICE ASSY., OIL CONTROL
18 O-RING, 10.8X2.4 (ARAI)
19 GAUGE COMP., OIL LEVEL
20 BOLT, FLANGE, 8X16
21 BOLT-WASHER, 6X10
22 BOLT-WASHER, 11X121
23 BOLT, DRAIN PLUG, 14MM
24 BOLT, MOUNTING BRACKET
25 BOLT, STUD, 6X28
26 BOLT, FLANGE, 6X20 (SEAL)
27 BOLT, DRAIN PLUG, 12MM
28 PIN, DOWEL, 15X22
29 PIN, DOWEL, 13X20
30 OIL SEAL, 80X100X10 (ARAI)
30 OIL SEAL, 80X100X10 (NOK)
31 O-RING, 28.7X3.5
32 PACKING, BEARING CAP BRIDGE (ARAI)
33 BOLT-WASHER, 6X16
34 NUT, FLANGE, 6MM
35 WASHER, DRAIN PLUG, 12MM
36 WASHER, DRAIN PLUG, 14MM
37 PIN, DOWEL, 10X16
38 PIN, DOWEL, 12X20
39 PIN, DOWEL, 6X10
40 BOLT, FLANGE, 6X16
41 BOLT, FLANGE, 6X18
42 BOLT, FLANGE, 10X40
43 BOLT, FLANGE, 10X50
44 BOLT, FLANGE, 10X55