PREVIOUS | INDEX |

2 PLUG, FUSIBLE (SAK)
3 O-RING (3/8")
4 O-RING (5/8")
5 CLIP, RECEIVER PIPE
6 GROMMET, SUCTION PIPE
7 GROMMET, LIQUID PIPE
8 HOSE COMP., SUCTION
9 HOSE COMP., DISCHARGE
10 PIPE, CONDENSER (SAK)
11 PIPE A, RECEIVER (SAK)
12 PIPE B, RECEIVER
13 PIPE D, RECEIVER (SAK)
14 TANK ASSY., RECEIVER
15 BRACKET, RECEIVER TANK
16 STAY A, SUCTION HOSE
17 CLAMP B, HOSE SOCKET
20 CLAMP, DISCHARGE HOSE
21 CLAMP, RECEIVER PIPE
22 CLAMP, SUCTION HOSE
23 CLAMP, HOSE SOCKET
24 CLAMP A, DISCHARGE HOSE
25 CLAMP B, RECEIVER PIPE
26 CLAMP C, RECEIVER PIPE
27 CLIP A, RECEIVER PIPE
28 SWITCH, DUAL PRESSURE
29 GROMMET, SCREW, 6MM
30 O-RING (1/2")
31 CLAMP, HOSE
32 CAP, VALVE (SAK)
34 BOLT-WASHER, 6X16
35 BOLT-WASHER, 6X16
36 BOLT-WASHER, 6X20
37 BOLT-WASHER, 8X35
38 SCREW, TAPPING, 6X16