PREVIOUS | INDEX |

1 TUBE COMP. A, BREATHER
2 CLAMP, FUEL HOSE
3 VALVE ASSY., PCV
4 PIPE COMP., BREATHER
5 TUBE, BREATHER PIPE (B)
6 GROMMET, PCV VALVE
7 JOINT, BREATHER THREE WAY
8 JOINT B, BYPASS THREE WAY
9 PUMP COMP., WATER
10 PACKING, WATER PUMP
11 THERMOSTAT UNIT (82) (FUJI SEIKO)
11 THERMOSTAT UNIT (82) (NIPPON THERMOSTAT)
11 THERMOSTAT UNIT (88) (FUJI SEIKO)
11 THERMOSTAT UNIT (88) (NIPPON THERMOSTAT)
12 RUBBER, THERMOSTAT MOUNTING
13 COVER, THERMOSTAT
14 GASKET, THERMOSTAT CASE
15 CASE COMP., THERMOSTAT
16 CLAMP, FAST IDLE CONTROL HOSE
17 HOSE, BYPASS IN.
18 PIPE COMP., CONNECTING
19 HOSE B, BYPASS
20 HOSE A, FAST IDLE CONTROL
21 HOSE B, FAST IDLE CONTROL
22 HOSE A, ELECTRONIC IDLE CONTROL VALVE
23 HOSE B, BYPASS INLET
24 CLIP, HOSE, 18.7MM
25 CLIP, HOSE, 18.7MM
26 HOSE B, ELECTRONIC IDLE CONTROL VALVE
27 HOSE A, BREATHER HEATER
28 HOSE B, BREATHER HEATER
29 BOLT, BREATHING WATER
30 JOINT, TUBE
31 HOSE, OIL COOLER (A)
32 HOSE, OIL COOLER (B)
33 BOLT, FLANGE, 8X16
34 O-RING, 31.2X4.1 (NOK)
35 CLAMP, TUBE (D12)
36 CLAMP, TUBE (D17)
37 NUT, FLANGE, 8MM
38 CLAMP, TUBE (D12)
39 CLAMP, TUBE (D12.5)
40 BOLT, FLANGE, 6X25
41 BOLT, FLANGE, 6X45
42 BOLT, FLANGE, 6X10
43 BOLT, FLANGE, 6X25