PREVIOUS | INDEX | NEXT

1 COUNTERSHAFT COMP.
2 GEAR, COUNTERSHAFT LOW
3 GEAR, COUNTERSHAFT SECOND
4 GEAR, COUNTERSHAFT FIFTH
5 GEAR, COUNTERSHAFT THIRD
6 GEAR, COUNTERSHAFT FOURTH
7 SLEEVE SET, SYNCHRONIZER (1-2)
8 COLLAR A, DISTANCE, 36X44X29 (+0.05/+0.03)
8 COLLAR B, DISTANCE, 36X44X29 (0.00/-0.02)
9 WASHER A, 40X54X1.96
9 WASHER B, 40X54X1.99
9 WASHER C, 40X54X2.02
9 WASHER D, 40X54X2.05
9 WASHER E, 40X54X2.08
10 WASHER, SPRING, 23MM
11 NUT, HEX., 23MM
12 RING, SNAP, 56MM
13 BEARING, SPECIAL BALL (NTN)
14 BEARING, NEEDLE, 25X56.4X19
15 BEARING, NEEDLE, 40X46X27
16 BEARING, NEEDLE, 44X50X24 (TOYO)
17 DAMPER, FRICTION
18 DAMPER, FRICTION (LOW)