PREVIOUS | INDEX | NEXT

1 PLUG, SETTING HOLE
2 GROMMET A, SIDE PANEL, 23MM
3 CAP, FLOOR HOLE, 53MM
4 INSULATOR B, SIDE SILL HOLD
5 COVER, HOOD SIDE
6 INSULATOR, PILLAR LOWER
7 GROMMET, DRAIN HOLE, 25MM
8 PLUG, AUTO CRUISE
10 PLUG, BAFFLE PLATE
12 PLUG, HOLE
15 PLUG, COATING HOLE, 25MM
16 PLUG, FLOOR HOLE
17 GROMMET, WAX HOLE, 25MM
18 PLUG, ID PLATE HOLE, 4.4MM
19 PLUG, HOLE, 8MM
20 GROMMET, HEATER LEVER HOLE (20MM)
21 SEAL, R. FR. PILLAR INNER LOWER
23 SEAL, L. FR. PILLAR INNER LOWER
24 SEAL, RR. PILLAR UPPER (50X70)
25 PLUG, HOLE, 10MM
26 PLUG, BLIND, 7MM
27 PLUG, BLIND, 8MM
28 PLUG, BLIND, 10MM
29 PLUG, BLIND, 12MM
30 PLUG, BLIND, 15MM
31 PLUG, BLIND, 18MM
32 PLUG, BLIND, 20MM
33 PLUG, BLIND, 25MM
34 PLUG, BLIND, 35MM