PREVIOUS | INDEX | NEXT

1 COLUMN ASSY., STEERING (NIPPON SEIKO)
2 HOLDER B, STEERING COLUMN (LH)
3 COLLAR, STEERING RETAINER
5 COVER, STEERING JOINT
6 GUARD, STEERING JOINT
7 JOINT COMP. B, STEERING
8 CLIP A, JOINT COVER
9 CLIP B, JOINT COVER
10 PLATE, JOINT COVER
12 DUST SEAL COMP., JOINT
14 COVER ASSY., COLUMN UPPER *NH1L*
15 COVER, COLUMN UPPER *NH1L*
16 LABEL, TILT STEERING
17 LABEL, IGNITION INFORMATION
18 COVER, COLUMN LOWER *NH1L*
19 RING, COLUMN COVER
20 SCREW, TAPPING, 4X16
21 BOLT, STEERING YOKE, 8X28 (NIPPON SEIKO)
22 BOLT-WASHER, 8X35
23 WASHER, PLAIN, 8MM
24 WASHER, LOCK
25 BOLT-WASHER, 6X16
26 SCREW-WASHER, 5X12
27 NUT-WASHER, 8MM