PREVIOUS | INDEX | NEXT

1 RING SET, PISTON (STD.) (TEIKOKU)
1 RING SET, PISTON (STD.) (RIKEN)
1 RING SET, PISTON (OS 0.25) (TEIKOKU)
1 RING SET, PISTON (OS 0.25) (RIKEN)
1 RING SET, PISTON (OS 0.50) (TEIKOKU)
1 RING SET, PISTON (OS 0.50) (RIKEN)
2 PISTON A
2 PISTON B
2 PISTON (OS 0.25)
2 PISTON (OS 0.50)
3 PIN, PISTON
4 NUT, CONNECTING ROD
5 ROD COMP., CONNECTING
6 BEARING A, CONNECTING ROD (BLUE) (DAIDO)
6 BEARING A, CONNECTING ROD (BLUE) (TAIHO)
6 BEARING B, CONNECTING ROD (BLACK) (DAIDO)
6 BEARING B, CONNECTING ROD (BLACK) (TAIHO)
6 BEARING C, CONNECTING ROD (BROWN) (DAIDO)
6 BEARING C, CONNECTING ROD (BROWN) (TAIHO)
6 BEARING D, CONNECTING ROD (GREEN) (DAIDO)
6 BEARING D, CONNECTING ROD (GREEN) (TAIHO)
6 BEARING E, CONNECTING ROD (YELLOW) (DAIDO)
6 BEARING E, CONNECTING ROD (YELLOW) (TAIHO)
6 BEARING F, CONNECTING ROD (PINK) (DAIDO)
6 BEARING F, CONNECTING ROD (PINK) (TAIHO)
6 BEARING G, CONNECTING ROD (RED) (DAIDO)
6 BEARING G, CONNECTING ROD (RED) (TAIHO)
7 BOLT, CONNECTING ROD
8 CRANKSHAFT COMP.
9 BEARING A, MAIN (BLUE) (DAIDO)
9 BEARING A, MAIN (BLUE) (TAIHO)
9 BEARING B, MAIN (BLACK) (DAIDO)
9 BEARING B, MAIN (BLACK) (TAIHO)
9 BEARING C, MAIN (BROWN) (DAIDO)
9 BEARING C, MAIN (BROWN) (TAIHO)
9 BEARING D, MAIN (GREEN) (DAIDO)
9 BEARING D, MAIN (GREEN) (TAIHO)
9 BEARING E, MAIN (YELLOW) (DAIDO)
9 BEARING E, MAIN (YELLOW) (TAIHO)
9 BEARING F, MAIN (PINK) (DAIDO)
9 BEARING F, MAIN (PINK) (TAIHO)
9 BEARING G, MAIN (RED) (DAIDO)
9 BEARING G, MAIN (RED) (TAIHO)
10 WASHER, THRUST (DAIDO)
11 PULLEY, TIMING BELT DRIVE
12 PLATE, TIMING BELT GUIDE
13 PULLEY, CRANKSHAFT
14 BOLT, SPECIAL, 14MM (SAGA)
15 WASHER, 14.5X36X8
16 KEY, 4.5X11.0