PREVIOUS | INDEX | NEXT

1 BEARING ASSY., FR. HUB (TOYO SEIKO)
2 RING, FR. KNUCKLE
3 HUB ASSY., FR.
4 DISK, FR. BRAKE
5 GUARD, FR. SPLASH
6 KNUCKLE COMP., R. FR. (ABS)
7 PROTECTOR, KNUCKLE
8 KNUCKLE COMP., L. FR. (ABS)
9 JOINT COMP., LOWER BALL
10 BOOT, LOWER BALL DUST (MUSASHI)
11 JOINT COMP., FR. UPPER BALL
12 ARM ASSY., R. FR. UPPER
13 ARM ASSY., L. FR. UPPER
14 BOLT, UPPER ARM
15 CIRCLIP, UPPER BALL JOINT
16 BOOT, TIE ROD END (MUSASHI)
17 BOLT, WHEEL (TOKAI TRW)
17 BOLT, WHEEL (NAGOYA RASHI)
18 BOLT-WASHER, 6X12
19 NUT, SELF-LOCK, 10MM (SATO RASHI)
20 NUT, SELF-LOCK, 12MM (SATO RASHI)
21 NUT, SPINDLE (24MM)
22 NUT, UPPER BALL PIN, 10MM
23 NUT, CASTLE, 12MM
24 CIRCLIP, EXTERNAL, 40MM
25 CIRCLIP, INTERNAL, 78MM
26 CIRCLIP, FR. UPPER (MUSASHI)
27 SCREW, FLAT, 6X14
28 SCREW-WASHER, 6X14
29 PIN, SPLIT, 2.0X18
30 PIN, SPLIT, 3.0X22