PREVIOUS | INDEX | NEXT

1 HOLDER COMP., DRIVEN
2 O-RING, RACK GUIDE (YAMADA)
3 SPRING, RACK GUIDE PRESSURE
4 SCREW, RACK GUIDE
5 GUIDE, STEERING RACK
6 DUST SEAL, STEERING PINION
7 BAND, DRIVEN PINION
8 NUT, RACK SCREW LOCK
9 COVER, PINION DUST
10 HOUSING SUB ASSY., STEERING GEAR BOX
11 RETAINER, PACKING
12 CAP, CYLINDER
13 WASHER, RETAINER
14 PORT, ORIFICE
15 PINION, STEERING
16 CAP, GEAR BOX HOUSING
17 RING, PISTON SEAL (NOK)
18 BUSHING B, STEERING RACK
19 PACKING, CYLINDER END (NOK)
20 CLIP, BUSH STOPPER
21 BODY UNIT, VALVE
22 PORT COMP., VALVE
23 CAP, VALVE BODY
24 SPOOL COMP. B, CUT-OFF (-0.005 / 0)
25 SPRING, CUT-OFF
26 ORIFICE, SENSOR
27 ORIFICE, DAMPING
28 SEAL, PORT
29 PLUNGER (DIAMETER=7MM)
30 SPRING, RETURN
31 HOUSING B, FR. GEAR
32 BARREL, CYLINDER
33 RETAINER, RACK BUSH
34 SCREW, CYLINDER END
35 PINION COMP., DRIVEN (LH)
36 RACK COMP., STEERING (4WS)
37 WASHER, DRIVEN HOLDER
38 SPRING, CYLINDER
39 BUSHING A, STEERING RACK
40 SEAL, DRIVEN DUST
41 CAP, DRIVEN PINION
42 COLLAR, DRIVEN PINION
43 RING, DRIVEN PINION SEAL
44 MAGNET COMP., POWER STEERING
45 SCREW, DRIVEN CAP
46 BOLT, DRIVEN PLUG
47 CIRCLIP, SPECIAL, (EX22)
48 BOLT, DRIVEN HOLDER
49 BOLT, POWER STEERING CYLINDER
50 WASHER, SEALING (8MM)
51 RING, SNAP, 31MM
52 CIRCLIP, INTERNAL, 28MM
53 CIRCLIP, EXTERNAL, 30MM
54 BEARING, 6906Z
55 BEARING, RADIAL BALL, 6001Z
56 PIN, DOWEL, 8X10
57 ROLLER, 3.5X29.8
58 SEAL, DRIVEN PINION (NOK)
58 SEAL, DRIVEN PINION (ARAI)
59 O-RING, 3.4MM (ARAI)
59 O-RING, 3.4MM (NOK)
60 O-RING, 9.8X1.9 (NOK)
61 O-RING, 11X1.9 (ARAI)
62 O-RING, 27.5X2 (NOK)
62 O-RING, 27.5X2 (ARAI)
63 O-RING, 46X1.5 (ARAI)
63 O-RING, 46X1.5 (NOK)
64 O-RING, 45.5X2 (ARAI)
64 O-RING, 45.5X2 (NOK)
65 O-RING, 33.5X2.4 (NOK)
65 O-RING, 33.5X2.4 (ARAI)
66 O-RING, 19.8X1.9 (NOK)
66 O-RING, 19.8X1.9 (ARAI)
67 O-RING, 41X2.0 (NOK)
67 O-RING, 41X2.0 (ARAI)
68 O-RING, 35.5X2.4 (NOK)
68 O-RING, 35.5X2.4 (ARAI)
69 O-RING, 38.8X1.9 (NOK)
69 O-RING, 38.8X1.9 (ARAI)
70 O-RING, 39X1.5 (NOK)
70 O-RING, 39X1.5 (ARAI)
71 O-RING, 49.5X2.0 (NOK)
71 O-RING, 49.5X2.0 (ARAI)
72 O-RING, 53.5X2.0 (NOK)
72 O-RING, 53.5X2.0 (ARAI)
73 CIRCLIP, EXTERNAL, 12MM
74 BOLT, FLANGE, 6X60
75 BOLT, FLANGE, 6X18
76 BOLT, FLANGE, 6X22
77 ROLLER, 6X10