PREVIOUS | INDEX | NEXT

1 MAINSHAFT COMP.
2 SHAFT, REVERSE IDLE GEAR
3 GEAR, MAINSHAFT THIRD
4 GEAR, MAINSHAFT FOURTH
5 GEAR COMP., REVERSE IDLE
6 GEAR, MAINSHAFT FIFTH
7 SLEEVE SET, SYNCHRONIZER (3-4)
8 SLEEVE SET, SYNCHRONIZER (5)
9 RING, BLOCKING (50S)
10 RING, BRAKE STOPPER
11 RING, TAPER CONE
12 SPRING, SYNCHRONIZER (50MM)
13 COLLAR, DISTANCE, 28X37X15
14 COLLAR, DISTANCE, 31X38X56.5
15 WASHER, SPRING, 28MM
16 WASHER, 28MM
17 BOLT, SPECIAL, 10X31.5
18 WASHER, DRAIN PLUG, 10MM
19 BEARING, SPECIAL BALL, 63/28C
20 BEARING, BALL, 28X78X20
21 BEARING, NEEDLE, 38X43X26 (NTN)
22 BEARING, NEEDLE, 37X42X15
22 BEARING, NEEDLE, 37X42X14.8 (NTN)
23 PIN, SPRING, 4X8