PREVIOUS | INDEX | NEXT

1 GEAR, DRIVE PINION
2 GEAR, FINAL DRIVEN
3 CASE COMP., DIFFERENTIAL
4 SHAFT, PINION
5 GEAR, DIFFERENTIAL PINION
6 WASHER A, DIFFERENTIAL PINION (0.7MM)
WASHER B, DIFFERENTIAL PINION (0.8MM)
WASHER C, DIFFERENTIAL PINION (0.9MM)
WASHER D, DIFFERENTIAL PINION (1.0MM)
WASHER E, DIFFERENTIAL PINION (0.75MM)
WASHER F, DIFFERENTIAL PINION (0.85MM)
WASHER G, DIFFERENTIAL PINION (0.95MM)
7 SHIM A, 76MM (1.20)
SHIM AA, 76MM (1.98)
SHIM B, 76MM (1.23)
SHIM BB, 76MM (2.01)
SHIM C, 76MM (1.26)
SHIM CC, 76MM (2.04)
SHIM D, 76MM (1.29)
SHIM DD, 76MM (2.07)
SHIM E, 76MM (1.32)
SHIM F, 76MM (1.35)
SHIM G, 76MM (1.38)
SHIM H, 76MM (1.41)
SHIM I, 76MM (1.44)
SHIM J, 76MM (1.47)
SHIM K, 76MM (1.50)
SHIM L, 76MM (1.53)
SHIM M, 76MM (1.56)
SHIM N, 76MM (1.59)
SHIM O, 76MM (1.62)
SHIM P, 76MM (1.65)
SHIM Q, 76MM (1.68)
SHIM R, 76MM (1.71)
SHIM S, 76MM (1.74)
SHIM T, 76MM (1.77)
SHIM U, 76MM (1.80)
SHIM V, 76MM (1.83)
SHIM W, 76MM (1.86)
SHIM X, 76MM (1.89)
SHIM Y, 76MM (1.92)
SHIM Z, 76MM (1.95)
8 SHIM, 80MM
9 PLATE, DIFFERENTIAL SIDE
10 BOLT, SPECIAL, 10MM
11 WASHER, THRUST, 28X50X1.5
12 BEARING, TAPER, 30208 (KOYO)
13 BEARING, TAPER, 40X76.2 (KOYO)
14 PIN, SPRING, 4X32